// 
// Twitch View データ収集モジュール
//
//Startup=Show			// Show|Visible or Hide ... NVから起動した場合の表示モード 

// ボーレート(19200)，パリティ(none)，ストップビット(1)，データビット長(8)で固定
Port=COM3

// データは，ASCIIテキストとして いわゆる垂れ流し
// KeepAlive Packet は，24byte
// Data Packet は，74byte いずれも 行末のLF,CRを含む
// Twitch View 本体の RJ-45端子からシリアルデータ出力
// Ciscoなどのケーブルと異なり，特殊な配線割り当て
// 専用ケーブルとシリアルポートとの接続は，通常のクロスケーブルでOK

// 以下測定項目
//[ITEM]
//0:1=StartCharacter
//1:20=20 digit unique device identifier
//21:4=Software Revision
25:1=mode,TOF|PTC|ST|Tetanus|EventMarker   // Stimulus Mode
26:2=@mode,TOFcnt|PTCcnt|STcnt|
28:3=@mode,TOFrat|||    // TOF Ratio(0-199), not active 000
//31:1=    // 0 if Supramax has been set, 1 if not
32:2=Stim,mA  // (00-80) Stimulating current in mA, 00 if Event Marker
34:1=PulseWidth, |100|200|300  // 0 if Event Marker
35:1=Electrode // 0:Electrode 1, 1:Electrode 2
36:4=T1auc // AUC of first pulse 0-9999(TOF) or hight of ST; 0000 if PTC or Event Marker
40:4=T2auc // AUC of second pulse, 0000 if ST or PTC or Event Marker
44:4=T3auc // AUC of third pulse, 0000 if ST or PTC or Event Marker
48:4=T4auc // AUC of fourth pulse, 0000 if ST or PTC or Event Marker
52:4=CALauc //AUC of calibration (supramax pulse), 0000 if not set
56:6=datemonth // The date as (MMDDYY) or 000000
62:6=time  // The time in 24-hour format HHMMSS
//68:3=    // Unused Characters 000
//71:1=EOC // The character '#'   end of character
